# synthetic export generated by MikrotikManager
# generated-at: 2026-05-07T07:13:21.880Z

/system identity
set name="veesp.swe.rt.shx.su"

/interface
:put "interface name="ether1" mtu=1500 disabled=no"
:put "interface name="MSK-DC" mtu=1350 disabled=no"
:put "interface name="MSK-IHOR" mtu=1400 disabled=no"
:put "interface name="MSK-VPSVILLE" mtu=1400 disabled=no"
:put "interface name="NSK-SERVHOST" mtu=1400 disabled=no"
:put "interface name="br1" mtu=1500 disabled=no"
:put "interface name="gre-tunnel1" mtu=1450 disabled=no"
:put "interface name="lo" mtu=65536 disabled=no"
:put "interface name="wg-tunnel" mtu=1420 disabled=no"
:put "interface name="wg1" mtu=1280 disabled=no"

/ip address
add address=62.182.194.146/24 interface="ether1"
add address=10.200.100.26/30 interface="MSK-IHOR"
add address=10.200.200.2/30 interface="*5"
add address=10.200.40.2/30 interface="MSK-VPSVILLE"
add address=10.205.1.2/30 interface="wg1"
add address=10.200.100.2/30 interface="*11" comment="Interface: MSK-SELECTEL (GRE) to selectel.msk.rt.shx.su"
add address=10.200.100.38/30 interface="MSK-DC" comment="Interface: MSK-DC (GRE) to dc.msk.rt.shx.su"
add address=10.200.100.14/30 interface="MSK-VPSVILLE" comment="Interface: MSK-VPSVILLE (GRE) to vpsville.msk.rt.shx.su"
add address=10.101.1.2/30 interface="gre-tunnel1"
add address=10.200.100.54/30 interface="NSK-SERVHOST" comment="Interface: NSK-SERVHOST (GRE) to servhost.nsk.rt.shx.su"

/ip route
add dst-address=0.0.0.0/0 gateway=62.182.194.1 distance=1
add dst-address=10.101.1.0/30 gateway=gre-tunnel1 distance=0
add dst-address=10.200.100.12/30 gateway=MSK-VPSVILLE distance=0
add dst-address=10.200.100.24/30 gateway=MSK-IHOR distance=0
add dst-address=10.200.100.36/30 gateway=MSK-DC distance=0
add dst-address=10.200.100.52/30 gateway=NSK-SERVHOST distance=0
add dst-address=10.205.1.0/30 gateway=wg1 distance=0
add dst-address=62.182.194.0/24 gateway=br1 distance=0
add dst-address=192.168.0.0/16 gateway=10.200.100.13%MSK-VPSVILLE distance=1

/ip firewall filter
add chain=input action=drop protocol=udp dst-port=53
add chain=input action=accept protocol=udp dst-port=13231
