*filter

# default policy is DROP
-P INPUT DROP
-P OUTPUT DROP
-P FORWARD DROP

# forward ESP-tunneled traffic
-A FORWARD -i eth1 -m policy --dir in  --pol ipsec --proto esp -s PH_IP_CAROL -j ACCEPT
-A FORWARD -i eth1 -m policy --dir in  --pol ipsec --proto esp -s PH_IP_DAVE  -j ACCEPT
-A FORWARD -o eth1 -m policy --dir out --pol ipsec --proto esp -j ACCEPT

# clusterip rules
-A INPUT -i eth1 -d 192.168.0.5 -j CLUSTERIP --new --hashmode sourceip --clustermac 01:00:c0:a8:00:05 --total-nodes 1 --local-node 0 
-A INPUT -i eth0 -d 10.1.0.5    -j CLUSTERIP --new --hashmode sourceip --clustermac 01:00:0a:01:00:05 --total-nodes 1 --local-node 0 

# allow esp
-A INPUT  -p 50 -j ACCEPT
-A OUTPUT -p 50 -d PH_IP_CAROL -j ACCEPT
-A OUTPUT -p 50 -d PH_IP_DAVE -j ACCEPT

# allow esp on internal interface
-A OUTPUT -o eth0 -s PH_IP_ALICE -d PH_IP_MOON1 -p 50 -j ACCEPT

# allow IKE on internal interface
-A INPUT  -i eth0 -d PH_IP_ALICE -s PH_IP_MOON1 -p udp --sport 500 --dport 500 -j ACCEPT
-A OUTPUT -o eth0 -s PH_IP_ALICE -d PH_IP_MOON1 -p udp --dport 500 --sport 500 -j ACCEPT

# allow IKE
-A INPUT  -i eth1 -p udp --sport 500 --dport 500 -j ACCEPT
-A OUTPUT -o eth1 -p udp --dport 500 --sport 500 -j ACCEPT

# allow MobIKE
-A INPUT  -i eth1 -p udp --sport 4500 --dport 4500 -j ACCEPT
-A OUTPUT -o eth1 -p udp --dport 4500 --sport 4500 -j ACCEPT

# allow crl fetch from winnetou
-A INPUT  -i eth1 -p tcp --sport 80 -s PH_IP_WINNETOU -j ACCEPT
-A OUTPUT -o eth1 -p tcp --dport 80 -d PH_IP_WINNETOU -j ACCEPT

# allow heartbeat
-A INPUT  -i eth0 -d PH_IP_ALICE -s PH_IP_MOON1 -p udp --dport 4510 --sport 4510 -j ACCEPT
-A OUTPUT -o eth0 -s PH_IP_ALICE -d PH_IP_MOON1 -p udp --dport 4510 --sport 4510 -j ACCEPT

# allow ICMP type 3
-A INPUT  -i eth0 -d PH_IP_ALICE -s PH_IP_MOON1 -p icmp --icmp-type 3 -j ACCEPT
-A OUTPUT -o eth0 -s PH_IP_ALICE -d PH_IP_MOON1 -p icmp --icmp-type 3 -j ACCEPT

# allow IGMP multicasts
-A INPUT  -d 224.0.0.1 -p igmp -j ACCEPT
-A OUTPUT -s 224.0.0.1 -p igmp -j ACCEPT

# allow ssh
-A INPUT  -p tcp --dport 22 -j ACCEPT
-A OUTPUT -p tcp --sport 22 -j ACCEPT

COMMIT
