alice::ping6 -c 3 -W 1 -i 0.2 -s 8184 -p deadbeef ip6-bob.strongswan.org::8192 bytes from ip6-bob.strongswan.org.*: icmp_seq=3::YES
moon ::swanctl --list-sas --raw 2> /dev/null::gw-gw.*version=2 state=ESTABLISHED local-host=192.168.0.1 local-port=4500 local-id=moon.strongswan.org remote-host=192.168.0.2 remote-port=4500 remote-id=sun.strongswan.org initiator=yes.*nat-remote=yes nat-any=yes encr-alg=AES_CBC encr-keysize=256 integ-alg=HMAC_SHA2_384_192 prf-alg=PRF_HMAC_SHA2_384 dh-group=ECP_384.*child-sas.*net-net.*reqid=1 state=INSTALLED mode=TUNNEL protocol=ESP encap=yes.*encr-alg=AES_GCM_16 encr-keysize=256.*local-ts=\[fec1:\:/16\[ipv6-icmp]] remote-ts=\[fec2:\:/16\[ipv6-icmp]]::YES
sun  ::swanctl --list-sas --raw 2> /dev/null::gw-gw.*version=2 state=ESTABLISHED local-host=192.168.0.2 local-port=4500 local-id=sun.strongswan.org remote-host=192.168.0.1 remote-port=4500 remote-id=moon.strongswan.org.*nat-remote=yes nat-any=yes encr-alg=AES_CBC encr-keysize=256 integ-alg=HMAC_SHA2_384_192 prf-alg=PRF_HMAC_SHA2_384 dh-group=ECP_384.*child-sas.*net-net.*reqid=1 state=INSTALLED mode=TUNNEL protocol=ESP encap=yes.*encr-alg=AES_GCM_16 encr-keysize=256.*local-ts=\[fec2:\:/16\[ipv6-icmp]] remote-ts=\[fec1:\:/16\[ipv6-icmp]]::YES
sun::tcpdump::IP moon.strongswan.org.\(4500\|ipsec-nat-t\) > sun.strongswan.org.\(4500\|ipsec-nat-t\): UDP-encap: ESP::YES
sun::tcpdump::IP sun.strongswan.org.\(4500\|ipsec-nat-t\) > moon.strongswan.org.\(4500\|ipsec-nat-t\): UDP-encap: ESP::YES
