alice::ping -c 1 PH_IP_BOB::64 bytes from PH_IP_BOB: icmp_.eq=1::YES
venus::ping -c 1 PH_IP_BOB::64 bytes from PH_IP_BOB: icmp_.eq=1::YES
moon:: sleep 6::no output expected::NO
bob::  ping -c 1 PH_IP_ALICE::64 bytes from PH_IP_ALICE: icmp_.eq=1::YES
bob::  ping -c 1 PH_IP_VENUS::64 bytes from PH_IP_VENUS: icmp_.eq=1::YES
alice::swanctl --list-sas --raw 2> /dev/null::nat-t.*version=1 state=ESTABLISHED local-host=10.1.0.10 local-port=4500 local-id=alice@strongswan.org remote-host=192.168.0.2 remote-port=4500 remote-id=sun.strongswan.org initiator=yes.*nat-local=yes nat-any=yes encr-alg=AES_CBC encr-keysize=128 integ-alg=HMAC_SHA2_256_128 prf-alg=PRF_HMAC_SHA2_256 dh-group=CURVE_25519.*child-sas.*nat-t.*reqid=1 state=INSTALLED mode=TUNNEL protocol=ESP encap=yes.*encr-alg=AES_GCM_16 encr-keysize=128.*local-ts=\[10.1.0.10/32] remote-ts=\[10.2.0.0/16]::YES
venus::swanctl --list-sas --raw 2> /dev/null::nat-t.*version=1 state=ESTABLISHED local-host=10.1.0.20 local-port=4500 local-id=venus.strongswan.org remote-host=192.168.0.2 remote-port=4500 remote-id=sun.strongswan.org initiator=yes.*nat-local=yes nat-any=yes encr-alg=AES_CBC encr-keysize=128 integ-alg=HMAC_SHA2_256_128 prf-alg=PRF_HMAC_SHA2_256 dh-group=CURVE_25519.*child-sas.*nat-t.*reqid=1 state=INSTALLED mode=TUNNEL protocol=ESP encap=yes.*encr-alg=AES_GCM_16 encr-keysize=128.*local-ts=\[10.1.0.20/32] remote-ts=\[10.2.0.0/16]::YES
sun::  swanctl --list-sas --raw --ike-id 1 2> /dev/null::nat-t.*version=1 state=ESTABLISHED local-host=192.168.0.2 local-port=4500 local-id=sun.strongswan.org remote-host=192.168.0.1.*remote-id=alice@strongswan.org.*nat-remote=yes nat-any=yes encr-alg=AES_CBC encr-keysize=128 integ-alg=HMAC_SHA2_256_128 prf-alg=PRF_HMAC_SHA2_256 dh-group=CURVE_25519.*child-sas.*name=nat-t.*reqid=1 state=INSTALLED mode=TUNNEL protocol=ESP encap=yes.*encr-alg=AES_GCM_16 encr-keysize=128.*local-ts=\[10.2.0.0/16] remote-ts=\[10.1.0.10/32]::YES
sun::  swanctl --list-sas --raw --ike-id 2 2> /dev/null::nat-t.*version=1 state=ESTABLISHED local-host=192.168.0.2 local-port=4500 local-id=sun.strongswan.org remote-host=192.168.0.1.*remote-id=venus.strongswan.org.*nat-remote=yes nat-any=yes encr-alg=AES_CBC encr-keysize=128 integ-alg=HMAC_SHA2_256_128 prf-alg=PRF_HMAC_SHA2_256 dh-group=CURVE_25519.*child-sas.*name=nat-t.*reqid=2 state=INSTALLED mode=TUNNEL protocol=ESP encap=yes.*encr-alg=AES_GCM_16 encr-keysize=128.*local-ts=\[10.2.0.0/16] remote-ts=\[10.1.0.20/32]::YES
moon::tcpdump::IP moon.strongswan.org.* > sun.strongswan.org.\(4500\|ipsec-nat-t\): UDP-encap: ESP::YES
moon::tcpdump::IP sun.strongswan.org.\(4500\|ipsec-nat-t\) > moon.strongswan.org.*: UDP-encap: ESP::YES
moon::tcpdump::IP moon.strongswan.org.* > sun.strongswan.org.\(4500\|ipsec-nat-t\): isakmp-nat-keep-alive::YES
alice::cat /var/log/daemon.log::sending keep alive::YES
venus::cat /var/log/daemon.log::sending keep alive::YES
