carol::cat /var/log/daemon.log::performing a DNS query for IPSECKEY RRs of.*moon.strongswan.org::YES
carol::swanctl --list-sas --raw 2> /dev/null::home.*version=2 state=ESTABLISHED local-host=192.168.0.100 local-port=4500 local-id=carol.strongswan.org remote-host=192.168.0.1 remote-port=4500 remote-id=moon.strongswan.org initiator=yes.*encr-alg=AES_CBC encr-keysize=128 integ-alg=HMAC_SHA2_256_128 prf-alg=PRF_HMAC_SHA2_256 dh-group=CURVE_25519.*local-vips=\[10.3.0.1] child-sas.*home.*state=INSTALLED mode=TUNNEL protocol=ESP.*encr-alg=AES_GCM_16 encr-keysize=128.*local-ts=\[10.3.0.1/32] remote-ts=\[10.1.0.0/16]::YES
carol::cat /var/log/daemon.log::installing new virtual IP PH_IP_CAROL1::YES
carol::ping -c 1 PH_IP_ALICE::64 bytes from PH_IP_ALICE: icmp_.eq=1::YES
dave:: cat /var/log/daemon.log::performing a DNS query for IPSECKEY RRs of.*moon.strongswan.org::YES
dave:: swanctl --list-sas --raw 2> /dev/null::home.*version=2 state=ESTABLISHED local-host=192.168.0.200 local-port=4500 local-id=dave.strongswan.org remote-host=192.168.0.1 remote-port=4500 remote-id=moon.strongswan.org initiator=yes.*encr-alg=AES_CBC encr-keysize=128 integ-alg=HMAC_SHA2_256_128 prf-alg=PRF_HMAC_SHA2_256 dh-group=CURVE_25519.*local-vips=\[10.3.0.2] child-sas.*home.*state=INSTALLED mode=TUNNEL protocol=ESP.*encr-alg=AES_GCM_16 encr-keysize=128.*local-ts=\[10.3.0.2/32] remote-ts=\[10.1.0.0/16]::YES
dave:: cat /var/log/daemon.log::installing new virtual IP PH_IP_DAVE1::YES
dave:: ping -c 1 PH_IP_ALICE::64 bytes from PH_IP_ALICE: icmp_.eq=1::YES
moon:: cat /var/log/daemon.log::performing a DNS query for IPSECKEY RRs of.*carol.strongswan.org::YES
moon:: cat /var/log/daemon.log::performing a DNS query for IPSECKEY RRs of.*dave.strongswan.org::YES
moon:: swanctl --list-sas --ike-id 1 --raw 2> /dev/null::rw.*version=2 state=ESTABLISHED local-host=192.168.0.1 local-port=4500 local-id=moon.strongswan.org remote-host=192.168.0.100 remote-port=4500 remote-id=carol.strongswan.org.*encr-alg=AES_CBC encr-keysize=128 integ-alg=HMAC_SHA2_256_128 prf-alg=PRF_HMAC_SHA2_256 dh-group=CURVE_25519.*remote-vips=\[10.3.0.1] child-sas.*net.*state=INSTALLED mode=TUNNEL protocol=ESP.*encr-alg=AES_GCM_16 encr-keysize=128.*local-ts=\[10.1.0.0/16] remote-ts=\[10.3.0.1/32]::YES
moon:: swanctl --list-sas --ike-id 2 --raw 2> /dev/null::rw.*version=2 state=ESTABLISHED local-host=192.168.0.1 local-port=4500 local-id=moon.strongswan.org remote-host=192.168.0.200 remote-port=4500 remote-id=dave.strongswan.org.*encr-alg=AES_CBC encr-keysize=128 integ-alg=HMAC_SHA2_256_128 prf-alg=PRF_HMAC_SHA2_256 dh-group=CURVE_25519.*remote-vips=\[10.3.0.2] child-sas.*net.*state=INSTALLED mode=TUNNEL protocol=ESP.*encr-alg=AES_GCM_16 encr-keysize=128.*local-ts=\[10.1.0.0/16] remote-ts=\[10.3.0.2/32]::YES
moon::tcpdump::IP carol.strongswan.org > moon.strongswan.org: ESP::YES
moon::tcpdump::IP moon.strongswan.org > carol.strongswan.org: ESP::YES
moon::tcpdump::IP dave.strongswan.org > moon.strongswan.org: ESP::YES
moon::tcpdump::IP moon.strongswan.org > dave.strongswan.org: ESP::YES
alice::tcpdump::IP carol1.strongswan.org > alice.strongswan.org: ICMP echo request::YES
alice::tcpdump::IP alice.strongswan.org > carol1.strongswan.org: ICMP echo reply::YES
alice::tcpdump::IP dave1.strongswan.org > alice.strongswan.org: ICMP echo request::YES
alice::tcpdump::IP alice.strongswan.org > dave1.strongswan.org: ICMP echo reply::YES
